{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["零星修缮"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"零星修缮","index":0,"n_rows":191,"n_cols":6,"rows_kept":191,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,1],[2,2,2,5],[3,0,3,1],[3,2,3,5],[4,0,4,1],[4,2,4,5],[5,0,5,5],[7,1,7,5],[19,1,19,5],[20,1,20,5],[24,0,25,0],[24,1,25,1],[24,2,25,2],[24,3,25,3],[24,4,25,4],[28,0,29,0],[28,1,29,1],[28,2,29,2],[28,3,29,3],[28,4,29,4],[30,0,31,0],[30,1,31,1],[30,2,31,2],[30,3,31,3],[30,4,31,4],[32,0,33,0],[32,1,33,1],[32,2,33,2],[32,3,33,3],[32,4,33,4],[56,1,56,5],[57,0,58,0],[57,1,58,1],[57,2,58,2],[57,3,58,3],[57,4,58,4],[67,1,67,5],[79,1,79,5],[82,0,83,0],[82,1,83,1],[82,2,83,2],[82,3,83,3],[82,4,83,4],[87,1,87,5],[101,0,107,0],[101,1,107,1],[101,2,107,2],[101,3,107,3],[101,4,107,4],[108,1,108,5],[144,1,144,5],[168,0,171,0],[168,1,171,1],[168,2,171,2],[168,3,171,3],[168,4,171,4],[172,1,172,5],[173,0,174,0],[173,1,174,1],[173,2,174,2],[173,3,174,3],[173,4,174,4]]}
["建筑及室外设施零星修缮项目报价表"]
["注：\n一、请详细填写此份清单作为报价单，红色部分为报名供应商应填项；\n二、此份清单仅作为遴选时的对比参考，实际采购数量以院部在合同期限内的实际需求为准，包括但不限于此份清单的品类；\n三、中标后，以此报价表为合作价格依据，实际采购过程中超出此份清单品目的部分，需中标公司后期再进行报价增补；\n四、合作年限：1年\n五、此报价表所有信息请务必填写详细、完整。此表格（Excel格式电子版及纸质盖章版）也应一并提交。"]
["公司名称"]
["联系人和联系方式"]
["相关业务资质"]
["建筑及室外设施零星修缮项目报价表"]
["序号","项目名称","单位","要求","单价/元（含税价）","备注"]
["一","拆除项目"]
[1,"拆除水泥砂浆基层","㎡","含清理、外运、人工"]
[2,"拆除墙面原贴面瓷砖","㎡","含清理、外运、人工"]
[3,"拆除120厚砖墙","㎡","含清理、外运、人工"]
[4,"拆除180厚-240厚墙体","㎡","含清理、外运、人工"]
[5,"拆除天棚吊顶","㎡","含清理、外运、人工"]
[6,"拆除地面砖、石材","㎡","含清理、外运、人工"]
[7,"拆除板材水池洗手台","个","含清理、外运、人工"]
[8,"拆除原木作门、钢质门、防火门","樘","含清理、外运、人工"]
[9,"电动门玻璃拆除和安装","项","含清理、外运、人工"]
[10,"拆除原塑胶地板","㎡","含清理、外运、人工"]
[11,"切割砖墙120/240mm厚","㎡","含清理、外运、人工"]
["二","建筑设施"]
["（一）","墙面设施"]
[1,"120厚墙体砌筑大于5m2按面积计取，小于5m2按工日计取","㎡","含材料、二次搬运、人工"]
[2,"180厚墙体砌筑大于5m2按面积计取，小于5m2按工日计取","㎡","含材料、二次搬运、人工"]
[3,"240厚墙体砌筑大于5m2按面积计取，小于5m2按工日计取","㎡","含材料、二次搬运、人工"]
[4,"贴墙面瓷砖大于5m2按面积计取，小于5m2按工日计取","㎡","含材料、刷背胶、二次搬运、人工\n砖品牌：诺贝尔、东鹏、鹰牌等国内一线品牌。"]
[]
[5,"墙面水泥砂浆粉刷","㎡","含材料、二次搬运、人工"]
[6,"仿石材外墙漆","㎡","品牌：东方雨虹、三棵树、立邦（含材料、二次搬运、人工）"]
[7,"墙面、天棚涂料刷白","㎡","刷底漆一遍、乳胶漆二遍等\n品牌：美惠、立邦、三棵树。含辅材料、二次搬运、人工"]
[]
[8,"墙面、天棚批腻子粉","㎡","清扫、批腻子二遍、打磨\n品牌：美惠、立邦、三棵树。含辅材料、二次搬运、人工"]
[]
[9,"墙面肌理漆面漆","㎡","刷底漆、面漆、罩面漆\n品牌：七彩龙、多乐士、泰诗尔。含辅材料、二次搬运、人工"]
[]
[10,"轻钢龙骨（75mm宽系列型材）","㎡","轻钢龙骨：龙牌、杰科、可耐福。（含材料、二次搬运、人工）"]
[11,"9mm厚石膏板双层(A级防火)","㎡","石膏板：泰山、杰科、可耐福。（含材料、二次搬运、人工）"]
[12,"9mm厚硅酸钙板双层(A级防火)","㎡","硅酸钙板：泰山、杰科、可耐福。（含材料、二次搬运、人工）"]
[13,"10mm厚埃特板(A级防火)","㎡","埃特板：龙牌、杰科、可耐福。（含材料、二次搬运、人工）"]
[14,"5mm木饰面","㎡","木饰面：兔宝宝、千年舟、莫干山。（含材料、二次搬运、人工）"]
[15,"8mm集成板(B级防火)","㎡","集成板：龙牌、杰科、可耐福。（含材料、二次搬运、人工）"]
[16,"6mm无机预涂板(A级)墙面","㎡","含材料、二次搬运、人工"]
[17,"玻镁彩钢板隔墙（50mm厚）","㎡","品牌：新太、荣盛、康星（含材料、二次搬运、人工）"]
[18,"电解钢板模块化饰面","㎡","含材料、二次搬运、人工"]
[19,"人造石 柱面板（25mm厚）","㎡","含材料、二次搬运、人工"]
[20,"18mm人造石英石板材","㎡","含材料、二次搬运、人工"]
[21,"工作台生态板18mm柜（宽600*高800mm）","m","含材料、二次搬运、人工"]
[22,"干挂铝板2.0mm厚墙面","㎡","含材料、二次搬运、人工"]
[23,"3公分外墙石板材干挂","㎡","含材料、二次搬运、人工"]
[24,"外墙石板材干挂钢结构","㎡","铁件加工，钢架制作、安装、焊接等全部操作过程。含材料、二次搬运、人工"]
[25,"50mm厚岩棉防火板隔墙","㎡","品牌：金钜、卫盾、易众洁（含安装材料、二次搬运、人工等）"]
[26,"外墙干挂陶板","㎡","60头虾红，含材料、二次搬运、人工"]
[27,"铝合金圆弧角线","m","含材料、二次搬运、人工"]
[28,"铝合金踢脚线（60mm高）","m","含材料、二次搬运、人工"]
[29,"定制不锈钢踢脚线（100mm高）","m","含材料、二次搬运、人工"]
[30,"结构胶修复","m","主要用于外墙干挂石材、铝板墙面、雨棚玻璃等构造，含拆除、材料、二次搬运、人工(不含外架、高空)"]
[31,"瓷砖角线","m","含材料、二次搬运、人工"]
["（二）","地面设施"]
[1,"铺地板瓷砖大于5m2按面积计取，小于5m2按工日计取","㎡","含材料、刷背胶、二次搬运、人工\n瓷砖品牌：诺贝尔、东鹏、鹰牌等国内一线品牌。含材料、二次搬运、人工"]
[]
[2,"地面石材20mm厚烟雨蒙蒙(A级）","㎡","含材料、二次搬运、人工等"]
[3,"地面石材20mm厚云朵拉灰(A级）","㎡","含材料、二次搬运、人工等"]
[4,"C25混凝土","m³","含材料、二次搬运、人工"]
[5,"C30混凝土","m³","含材料、二次搬运、人工"]
[6,"地面自流平找平","㎡","品牌：德高、旺拉利、立邦（含材料、二次搬运、人工）"]
[7,"2.0厚PVC卷材地板（同质透心）","㎡","品牌：阿姆斯壮，洁福、得嘉等国内一线品牌（含材料、二次搬运、人工等）"]
[8,"地面水泥砂浆找平层","㎡","含材料、二次搬运、人工"]
[9,"门槛大理石","㎡","含材料、二次搬运、人工"]
["（三）","天棚设施"]
[1,"轻钢龙骨吊顶（75mm宽系列型材）","㎡","1、轻钢龙骨：龙牌、杰科、可耐福 2、含材料、二次搬运、人工"]
[2,"9mm厚硅酸钙板双层(A级防火)","㎡","1、硅酸钙板：龙牌、杰科、可耐福 、2.含材料、二次搬运、人工"]
[3,"9mm厚石膏板双层(A级防火）","㎡","石膏板：泰山、杰科、可耐福。（含材料、二次搬运、人工）"]
[4,"10mm厚埃特板(A级防火）","㎡","埃特板：龙牌、杰科、可耐福。（含材料、二次搬运、人工）"]
[5,"6mm厚无机预涂板(A级防火)","㎡","（含材料、二次搬运、人工）"]
[6,"12mm厚蜂窝铝板(A级防火)","㎡","蜂窝铝板：龙牌、杰科、可耐福。（含材料、二次搬运、人工）"]
[7,"12mm厚胶合板(B级防火）","㎡","泰山、千年舟、兔宝宝（含材料、二次搬运、人工）"]
[8,"铝扣板（1.5mm厚)吊顶300*300","㎡","1、轻钢龙骨：龙牌、杰科、可耐福2、铝板蓝天七色、方大、金边。含材料、二次搬运、人工"]
[9,"铝扣板（1.5mm厚)吊顶300*600","㎡","1、轻钢龙骨：龙牌、杰科、可耐福2、铝板蓝天七色、方大、金边。含材料、二次搬运、人工"]
[10,"铝扣板（1.5mm厚)吊顶600*600","㎡","1、轻钢龙骨：龙牌、杰科、可耐福2、铝板蓝天七色、方大、金边。含材料、二次搬运、人工"]
[11,"铝扣板（1.5mm厚)吊顶600*1200","㎡","1、轻钢龙骨：龙牌、杰科、可耐福2、铝板蓝天七色、方大、金边。含材料、二次搬运、人工"]
["（四）","防水设施"]
[1,"1.5mm厚高分子复合防水材料","㎡","品牌：东方雨虹、永安固、立邦（含材料、二次搬运、人工）"]
[2,"3mm厚SBS防水卷材","㎡","品牌：东方雨虹、永安固、立邦（含材料、二次搬运、人工）"]
[3,"防水涂料2mm厚","㎡","含材料二次搬运、人工，\n防水涂料品牌：德高、雨虹、立邦"]
[]
[4,"楼板漏水高压注浆","点","品牌：东方雨虹、德高、立邦（含材料小于1平方米）。含材料、二次搬运、人工"]
[5,"楼板大理石地面空鼓高压注浆","㎡","品牌：东方雨虹、德高、立邦（含材料小于2平方米）。含材料、二次搬运、人工"]
[6,"防水补漏打针注浆","颗","品牌：东方雨虹、德高、立邦（含材料、二次搬运、人工）"]
["（五）","门窗设施"]
[1,"玻璃门不锈钢手把（长1200mm）","套","含材料、二次搬运、人工"]
[2,"木纹铝合金窗把手","套","含材料、二次搬运、人工"]
[3,"卫生间铝合金钢化玻璃门","㎡","含门框、材料、二次搬运、人工"]
[4,"玻璃电动门","㎡","品牌：GMT、欧赛斯顿、松下、欧尼克、铸诚（成套成品含门机），含材料、二次搬运、人工"]
[5,"钢制电动门","㎡","品牌：GMT、欧赛斯顿、松下、欧尼克、铸诚（成套成品含门机），含材料、二次搬运、人工"]
[6,"电动门电机","个","品牌：GMT、欧赛斯顿、松下、欧尼克（含材料、二次搬运、人工）"]
[7,"岩棉防火板门","㎡","品牌：美心、王力、天宏（含材料、门框灌浆、符合消防、医院相关规范要求（含材料、门框灌浆、二次搬运、人工等））"]
[8,"甲级防火门","㎡","品牌：美心、秀星、天宏（符合消防、医院相关规范要求（含辅材料、门框灌沙浆、二次搬运、人工等））"]
[9,"甲级防火门(有防火玻璃观察窗400*400）","㎡","品牌：美心、秀星、天宏（符合消防、医院相关规范要求（含辅材料、门框灌沙浆、二次搬运、人工等））"]
[10,"乙级防火门","㎡","品牌：美心、秀星、天宏（符合消防、医院相关规范要求（含辅材料、门框灌沙浆、二次搬运、人工等））"]
[11,"乙级防火门(有防火玻璃观察窗400*400）","㎡","品牌：美心、秀星、天宏（符合消防、医院相关规范要求（含辅材料、门框灌沙浆、二次搬运、人工等））"]
[12,"定制超规格甲级防火门","㎡","符合消防、医院相关规范要求:1、门框、门扇采用1.2mm厚电解板；\n2、门扇内框增加50*50*2.0mm镀锌方管；\n3、门框内框增加75*40*2.0mm镀锌方管（含材料、门框灌浆、二次搬运、人工等）"]
[13,"定制超规格甲级防火门（用于地下室、屋面）","㎡","符合消防、医院相关规范要求:1、门框、门扇采用1.2mm厚电解板；\n2、门扇内框增加50*50*2.0mm镀锌方管；\n3、门框内框增加75*40*2.0mm镀锌方管（含材料、门框灌浆、二次搬运、人工等）                      \n4、门框、门扇防生锈处理"]
[14,"钢制门","㎡","1、满足防污、抗菌的要求；\n2、门扇板要求：厚度≥0.8mm的优质热镀锌钢板，表面静电喷涂，喷涂前均需磷化处理；\n3、门框板要求：厚度≥1.5mm优质热镀锌钢板，表面静电喷涂，喷涂前均需磷化处理；\n4、 门扇采用一体折弯成型，无焊接点工艺，表面光滑美观、不变形，门扇内部采用先进绿色环保填充物，使门具有良好的密封和保温隔音效果，隔音性能达到28dB或以上；                                                                \n5、把手、锁具：304#不锈钢医院相应类别（病房、卫生间等）专用锁及把手；\n6、铰链：304#不锈钢蝶式铰链；\n7、紧固件（螺丝等）：材质需为304#不锈钢；（含材料、二次搬运、人工等）"]
[]
[]
[]
[]
[]
[]
["（六）","水电设施"]
[1,"LED平板灯600*600","盏","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[2,"LED平板灯300*600","盏","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[3,"LED平板灯开孔","个","含材料、二次搬运、人工"]
[4,"一开开关面板","块","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[5,"二开开关面板","块","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[6,"三开开关面板","块","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[7,"四开开关面板","块","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[8,"一开带五孔面板","块","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[9,"漏电保护空气开关63A","个","含材料、二次搬运、人工（西门子、ABB、施耐德）"]
[10,"漏电保护空气开关20A","个","含材料、二次搬运、人工（西门子、ABB、施耐德）"]
[11,"网络插座","个","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[12,"10孔10A插座（118型）","个","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[13,"五孔插座","个","含材料、二次搬运、人工（三雄极光、欧普、雷士）"]
[14,"集成排气扇300*600mm（总功率64W照明:24W 换气:40W）","套","含材料、二次搬运、人工（九牧、箭牌、雷士）"]
[15,"水龙头","个","含材料、二次搬运、人工（九牧、箭牌、恒洁）"]
[16,"PPR20给水管","m","含材料、二次搬运、人工"]
[17,"PPR20给水管弯头","个","含材料、二次搬运、人工"]
[18,"PPR20给水管直接","个","含材料、二次搬运、人工"]
[19,"50排水管","m","含材料、二次搬运、人工"]
[20,"2.5mm²单芯电线（铜芯）","m","含套管、材料、二次搬运、人工（南平太阳、青岛汉缆、上海起帆）"]
[21,"4mm²单芯电线（铜芯）","m","含套管、材料、二次搬运、人工（南平太阳、青岛汉缆、上海起帆）"]
[22,"50-70铜头","个","含材料、二次搬运、人工"]
[23,"25-35铜头","个","含材料、二次搬运、人工"]
[24,"蹲位砌筑150mm高","个","含材料、二次搬运、人工"]
[25,"蹲便器（规格520*420*280mm）","个","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[26,"小便斗（壁挂感应）","个","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[27,"小便斗（落地感应）","个","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[28,"立柱洗手盆","套","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[29,"脚踏阀","套","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[30,"角阀（铜材质）","个","含材料、二次搬运、安装人工（九牧、箭牌、恒洁）"]
[31,"不锈钢地漏","个","含材料、二次搬运、安装人工"]
[32,"铸铁圆井盖800*35mm（国标）重型30吨","个","含材料、二次搬运、人工"]
[33,"铸铁方井盖1000*1000mm（国标）重型30吨","个","含材料、二次搬运、人工"]
[34,"铸铁方井盖1000*1500mm（国标）重型30吨","个","含材料、二次搬运、人工"]
[35,"铸铁方井盖1000*2000mm（国标）重型30吨","个","含材料、二次搬运、人工"]
["三","室外设施"]
[1,"100mm厚透水混凝土面层（C30，含一道面层封闭剂）","㎡","含材料、二次搬运、人工"]
[2,"150mm厚C30透水混凝土结构层","㎡","含材料、二次搬运、人工"]
[3,"150mm厚C25砼路面","㎡","含材料、二次搬运、人工"]
[4,"40mm厚细粒式AC-13改性沥青+60mm厚细粒式AC-16改性沥青路面","㎡","含材料、二次搬运、人工"]
[5,"C25构造柱及圈梁200高同墙宽，钢筋HRB400：4根12纵筋,8@200箍筋。","m","含材料、二次搬运、人工"]
[6,"人行道透水砖（300*300*50mm）","㎡","含材料、二次搬运、人工"]
[7,"路沿石（光面芝麻黑花岗岩圆角15°600*300*150mm","m","含材料、二次搬运、人工"]
[8,"光面芝麻黑花岗岩平路沿石倒圆角15° 200*600*50mm","m","含材料、二次搬运、人工"]
[9,"水沟盖板（烧面芝麻灰花岗岩600*300*30mm）","m","含材料、二次搬运、人工"]
[10,"水沟盖板（烧面芝麻灰花岗岩600*300*50mm）",null,"含材料、二次搬运、人工"]
[11,"5mm厚钢制水沟盖板，网格50*50mm（1000*300*50mm）","m","含材料、二次搬运、人工"]
[12,"5mm厚钢制水沟盖板，网格50*50mm（600*450*30mm）","m","含材料、二次搬运、人工"]
[13,"5mm厚钢制水沟盖板，网格50*50mm（600*300*40mm）",null,"含材料、二次搬运、人工"]
[14,"475mm*353mm*35mm车载型塑料植草格","㎡","含材料、二次搬运、人工"]
[15,"烧面芝麻灰花岗岩（广场铺装）300*600*30mm","㎡","含材料、二次搬运、人工"]
[16,"荔枝面黄金麻花岗岩（园路）300*300*30mm","㎡","含材料、二次搬运、人工"]
[17,"烧面芝麻黑花岗岩（园路）150*600*30mm","㎡","含材料、二次搬运、人工"]
[18,"烧面芝麻白花岗岩（园路）200*200*30mm","㎡","含材料、二次搬运、人工"]
[19,"花岗岩（广场铺装）300*600*20mm","㎡","含材料、二次搬运、人工"]
[20,"花岗岩（广场铺装）300*600*40mm","㎡","含材料、二次搬运、人工"]
[21,"仿石材涂料","㎡","品牌：东方雨虹、三棵树、立邦（含材料、二次搬运、人工）"]
[22,"成品车挡","个","含材料、二次搬运、人工"]
[23,"院区栏杆氟碳漆修复","㎡","黑色氟碳漆饰面（含安装材料、二次搬运、人工等）"]
[24,"院区栏杆","㎡","立杆80X80x5、25X15X3方通,横杆60X40X5方通，80X40X3椭圆管扶手，100X10厚钢板，栏杆1.45M高，黑色氟碳漆饰面（含安装材料、二次搬运、人工等）",{"$f":"_xlfn.DISPIMG(\"ID_DB7B5A5883D44A82A3053BD52ECC00E5\",1)","v":"=DISPIMG(\"ID_DB7B5A5883D44A82A3053BD52ECC00E5\",1)"}]
[]
[]
[]
["四","其它"]
[1,"防火门喷漆","㎡","打磨、除锈、补原子灰二遍\n品牌：美惠、立邦、三棵树、含材料、二次搬运、人工"]
[]
[2,"地面大理石面破损修复","㎡","含材料、二次搬运、人工"]
[3,"PVC卷材地板补焊缝","m","含材料、二次搬运、人工"]
[4,"镀锌板管道200*200*2mm","m","含材料、二次搬运、人工"]
[5,"空调风管与出风口烤漆连接构件（烤漆板2mm厚）","个","含材料、二次搬运、人工"]
[6,"金钢取孔","个","楼板、墙Ø200mm以下。含材料、二次搬运、人工"]
[7,"中沙","㎥","含材料、二次搬运、人工"]
[8,"自行走式升降机","台班","每台班8小时、升降高度≥16m"]
[9,"630型电动高处作业吊篮","台班","每台班8小时"]
[10,"自行曲臂式升降平台","台班","每台班8小时、升降高度8-20m"]
[11,"挖掘机200型","台班","每台班8小时"]
[12,"吊车16T","台班","每台班8小时"]
[13,"吊车25T","台班","每台班8小时"]
[14,"土建修缮普工及技工工资","工日","人工不含材料"]
[15,"水电技工工资","工日","人工不含材料"]
[16,"电焊工工资","工日","含焊条.机械.人工"]
[17,"环卫处专用车外运垃圾","车","农用车.含装车、外运"]